Workstation for DOS ODI Client

Introduction:
-------------
This document describes the procedure to setup the NetWare V3.X, V4.X,
5.0 workstation driver for D-Link DFE-690TXD CardBus PC Card.

Location of Driver:     \NWCLIENT\DLKRCB.COM


Getting Start:
--------------

  1. For the PC that installing EMM386.EXE in the CONFIG.SYS.
     Please make sure the memory range D000-D7FF is excluded.

     Ex:
         DEVICE=C:\DOS\EMM386.EXE NOEMS X=D000-D7FF

  2. Copy <PATH>\ENABLER\*.* files from released disk into your
     hard disk.                                           
     Ex:
         copy E:\ENABLER\*.* C:\ENABLER

  3. Add a line

     @CALL C:\ENABLER\CBEN.BAT

     on the first line of AUTOEXEC.BAT file.


Sample Configuration Files:
---------------------------
  STARTNET.BAT:
      LSL
      DLKRCB
      IPXODI
      NETX or VLM (VLM's for NetWare 4.x, 5.0)

  NET.CFG:
      LINK DRIVER DLKRCB

        MEDIUM MM  --where MM is one of AUTO, 10HALF, 10FULL, 100HALF,
                     and 100FULL, to specifiy the media type.

        BUSNO NN   --where NN is the PCI bus identifier of the PCI bus
                     which connects to the adapter.

        DEVICENO NN --where NN is the specific PCI BIOS device
                      identification number of the specified PCI adapter.

       [ or you can use "EtherID" to select a specific DFE-690TXD adapter:
        EtherID 006067NNNNNN --Where 006067NNNNNN specify a DFE-690TXD
                               adapter's node address. This is only
                               required when more than one DFE-690TXD
                               adapters exist on one system.
       ]


        FRAME Ethernet_802.2 --Specify frame type
        FRAME Ethernet_802.3
        FRAME Ethernet_SNAP
        FRAME Ethernet_II

        NetWare DOS Requester
        FIRST NETWORK DRIVE = F
        NETWARE PROTOCOL = NDS BIND
        PREFERRED SERVER = NW411


Setup Procedures for NetWare 3.12 Client :
------------------------------------------
   Before you start with the installation process, make sure that
   the adapter is properly installed and configured. Make sure
   that your NetWare workstation is properly installed.

   1. Copy DLKRCB.COM from the DFE-690TXD Driver Disk subdirectory
      EX:
          E:\NWCLIENT to your harddisk.

   2. Update STARTNET.BAT batch file as sample above

   3. Edit the NET.CFG file that you copied over. Edit the file per your
      requirements (see examples above). If there are two frame types
      listed, whichever frame type is listed first, that is the one that
      the  driver will load. See above for examples. The NET.CFG file
      should be in the same directory with the LSL.COM file.


Setup Procedures for NetWare 4.X, 5.0 Client with vlm:
------------------------------------------------------
   1. Make a new directory NWCLIENT(or other name) on C drive

   2. Copy <PATH>\NWCLIENT\*.* files from released disk to 
      C:\NWCLIENT\*.*

   3. Create STARTNET.BAT batch file as sample above

   4. Add a line "@CALL C:\NWCLIENT\STARTNET.BAT"(ingore symbol "")
      on the first line of AUTOEXEC.BAT file.
      

NOTE:
-----
   1. Be sure LASTDRIVE=Z in your CONFIG.SYS file for the
      network mappings to work properly.

   2. When you have multiple DFE-690TXD Adapters on your system:
      Use "BUSNO" and "DEVICENO" KEYWORD in NET.CFG to select which
      adapter to use with your netware client.(or you can use "EtherID")

                                                                 -- End --