This document contains information about D-Link DFE-690TXD CardBus PC Card 
driver for Macintosh Power Mac series.  We urge you to read this document 
to gain some understanding of this product. This document address the 
following topics:

*** The D-Link DFE-690TXD CardBus PC Card driver 
    does not support the HOT-SWAP functionality of a PC Card.
    Thus you must plug the PC Card into your system before booting and 
    should not remove the PC Card from your system before shuting down.
    PLEASE DO NOT HOT-SWAP THE PC CARD WHEN YOUR MAC SYSTEM IS RUNNING.

1. Adapter requirement for PC Card
2. Software Installation
3. Setting up Open Transport
4. Setting up the TCP/IP

1. Adapter requirement for PC Card
1.1 The NIC on your PC Card must be D-Link DFE-690TXD CardBus PC Card 
    series and the Vendor ID musb be 1186 and the Device ID must be 1340. 
       * You can contact your PC Card provider to get the Vendor ID 
         and Device ID of your PC Card. 
1.2 If the Vendor ID and Device ID is not 1186,1340, please contact 
    your PC Card provider to get the driver for your PC Card or follow
    the following steps to patch our driver to work with your PC Card.
      - Get a binary editor to edit the driver.
        *** You can use "General Edit Lite" editor You can download 
            "General Edit Lite" from 	
              ftp://physgi.phy.ncku.edu.tw/pub/mac/editor.
      - Use this editor to open the driver file "DFE690".
      - Select "Unlock Data" from the "View" menu item to unlock data
        of the driver file to enable the editor to modify the driver
        file.
      - Click on the lower frame to activate the lower frame.
      - Replace all the pci1186,1340 items with your pcixxxx,yyyy 
        whree xxxx is the Vendor ID and yyyy is the Device ID of your 
        PC Card by using the"Replace" function provided in the 
        "Replace" menu item in the "Find" menu item. 
      - Save the driver file.
    note: "Quadrivio General Edit Lite" is a product of Quadrivio
    corporation. 
    Please read the text file within the "Quadrivio General Edit Lite".
    You can contact Quadrivio corporation for more information.

2. Software Installation
2.1 Double-click the "Installer" 
    icon in the "DFE-690TXD Driver for Mac OS" folder. 
    The installer program examines your computer and installs the 
    appropriate driver according to your selection.

3. Setting up the AppleTalk Control Panel
3.1 Select the "Control Panels" from the Apple Menu.
3.2 Select "AppleTalk" from the Control Panels submeu. 
3.3 Click the "Connect via:" dropdown list box to show available 
    communication connections.
3.4 Select the slot where the adapter is installed.
3.5 Close the AppleTalk control panel. A dialog box will appear asking
    whether you want to save changes. Click the "Save" button.

4. Setting up the TCP/IP
4.1 Select "Control Panels" from the Apple Menu.
4.2 Select "TCP/IP" from te Control Panels submenu.
4.3 Click the "Connect via:" dropdown list box to show available 
    communication connections.
4.4 Select the slot where the adapter is installed.
4.5 Close the TCP/IP control panel. A dialog box will appear asking 
    whether you want to save changes. Click the "Save" button.
