Packet Driver

Introduction:
-------------
This document describes the procedure to setup the Packet driver for
D-Link DFE-690TXD CardBus PC Card.

   Location of Driver:     \PKTDRV\DLKRCB.COM

Getting Start:
--------------

  1. For the PC that installing EMM386.EXE in the CONFIG.SYS.
     Please make sure the memory range D000-D7FF is excluded.

     Ex:
         DEVICE=C:\DOS\EMM386.EXE NOEMS X=D000-D7FF

  2. Copy <PATH>\ENABLER\*.* files from released disk into your
     hard disk.                                                    
     Ex:                                                           
         copy E:\ENABLER\*.* C:\ENABLER                            

  3. Add a line

     @CALL C:\ENABLER\CBEN.BAT

     on the first line of AUTOEXEC.BAT file.

Notes:
------
  1.  Load the packet driver using the software interrupt and any
      optional switches if required.

      Usage: DLKRCB [options] <software_int_no> [media type]

      Example: DLKRCB -i 0x7e

      The only required parameter is the software interrupt. A packet
      driver needs to have a software interrupt assigned to it for other
      programs to access it. The recommended interrupt 0x7e. If you need
      any of the options listed below, place them before the software
      interrupt on the command line.

      -i - Force driver to report itself as 802.3 instead of Ethernet II.
      -d - Delayed initialization. Used for diskless booting
      -n - NetWare conversion. Converts 802.3 packets into 8137 packets
      -w - Windows hack, obsoleted by winpkt
      -p - Promiscuous mode disable
      -h - Help
      -u - Uninstall

   2. Media type can be used to force the card to work on specific
      speed and duplex mode. If no media type if specified, then
      driver will read hardware configuration from EEPROM on the
      card.

   3. Type command, C:\DLKRCB 0x60, the screen will appear following
      message:

      Packet driver for D-Link DFE-690TXD CardBus PC Card version 3.21
      Copyright , 2001 D-Link Corp. All Rights Reserved.

      Line Speed 100 Mbps
      Half Duplex
      System: [345]86 processor, PCI bus, Two 8259s
      Packet driver software interrupt is 0x60
      Interrupt number is 0xA
      I/O port is 0xE000
      My Ethernet address is 00:50:BA:D0:17:EB

   4. Installing Multiple LAN Adapters:

      If there are multiple network cards on the main board, the user
      run DLKRCB 0x60 directly, then the screen will display :

      Packet driver for D-Link DFE-690TXD CardBus PC Card version 3.21
      Copyright , 2001 D-Link Corp. All Rights Reserved.

      There are 2 network cards on your main board :
      Card 1. SlotNo= 0xA. IRQ= 0xC  I/O= 0xE000  NodeID= 00:50:BA:D0:17:31
      Card 2. SlotNo= 0xB. IRQ= 0xA  I/O= 0xD800  NodeID= 00:50:BA:D0:17:EB
      Please select a Card No.(1-2): 1

      Line Speed 100 Mbps
      Half Duplex
      System: [345]86 processor, PCI bus, Two 8259s
      Packet driver software interrupt is 0x60
      Interrupt number is 0xC
      I/O port is 0xE000
      My Ethernet address is 00:50:BA:D0:17:31

                                                                 -- End --