Von:	Lidin Gregory (GS-ES/EAS3) *
Gesendet:	Freitag, 4. Februar 2005 16:33
An:	Keller Thomas (GS-EC/ESI4) *; Borchert Andre (GS-EC/ESI4) *
Betreff:	ME711 Flashprogramming delivery

Delivery notification

The 4 versions of Ram-Pst for Me7 VW/Audi  ST10 projects has been updated. See the changes description bellow.

•	[FS : FP / ME711_VW_CANEXT; 3]
•	[FS : FP / ME711_VW_CANEXT_2SG; 2]
•	[FS : FP / ME711_VW_KLEXT; 3]
•	[FS : FP / ME711_VW_KLEXT_2SG; 3]

Delivery description :

Module Order	Type of change	Description  	
MO108722	S	Correction after custormer test 	
MO112993	S	Decomp bugfix	

MO108722 : details   see : [DOCU : MO108722_SRS / 1.10; 1]

Point in the customer test document	To do	
5.2	WSC Code must be updated during the flashprogrammming. That update must be visible in the running Ram-Pst session (Read ECU Id) and after programming, in drive.	
8.4	Test on format-Identifier more selective	
12.1	A wrong checksum result must return “KWP2000_DOWNLOADNOTEXPECTED”	
13.3	In Ram-Pst : Request download must be enabled only after SA. If Security access was done in Drive, the Seed must have been requested befor Request Dowload (Seed = 0 sent to the tester)	
13.4	Security access to improve. Lock the order Seed > Key. 	

Integration document :

[DOCU : FP_ME711_ST10_INT / 1.10; 0]

Test plan after integration

Short test to check the flashprogramming after the first integration. See the integration document for more details.

[DOCU : FP_ME711_ST10_TEST / 1.10; 0]

Official programming tools :

<<\\Si7274\K3pr_sgsw\003\Projekte\ME711\90_Tools\ME711 Prof Kline>>
<<\\Si7274\K3pr_sgsw\003\Projekte\ME711\90_Tools\ME711 Prof TP20>>

Grüss,
Grégory LIDIN
_________________________________________
Robert BOSCH France
Gasoline Systems - Software Development
Tél. : +33(1)4010-7489
________________________________________