;***********************************************************************
;
; NETIMWEB.INF
;
;   This installation script supports Windows 98, Me, 2000 & XP for the
;   High Rate Wireless LAN Mini-PCI Adapter with Modem II Adapter.
;
;   Copyright (c) 2003 Intel Corporation
;   All Rights Reserved.
;   
;
;***********************************************************************

[Version]
 DriverVer = 06/04/2003, 3.0.4.205
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
 CatalogFile         = NETIMWEB.cat
 MillenniumPreferred = .ME


[Manufacturer]
%VER_VENDOR_NAME_STR% = DeviceList,NTx86.5.1


[DeviceList.NTx86.5.1]
%IMWEB_PCI1_STR%        = IMWEB_PCI1.NT.5.1,PCI\VEN_1260&DEV_3873&SUBSYS_25138086	
;%IMWEB_PCI2_STR%        	

[DeviceList]
%IMWEB_PCI1_STR%   = IMWEB_PCI1,PCI\VEN_1260&DEV_3873&SUBSYS_25138086	
;%IMWEB_PCI2_STR%   


[ControlFlags]
;Exclude all PNP adapters from user selection
ExcludeFromSelect   = PCI\VEN_1260&DEV_3873&SUBSYS_25138086
	
;=========================================IMWEB_PCI1==========================================================================
[IMWEB_PCI1]            ; Win9x
 AddReg         = IMWEB_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = IMWEB_DRIVER.copy, IMWEB_APPLET.copy, IMWEB_NDI.copy

[IMWEB_PCI1.ME]         ; WinMe
 AddReg         = IMWEB_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = IMWEB_DRIVER.copy.ME, IMWEB_APPLET.copy.ME, IMWEB_NDI.copy.ME
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[IMWEB_PCI1.ME.ME]      ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = IMWEB_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = IMWEB_DRIVER.copy.ME, IMWEB_APPLET.copy.ME, IMWEB_NDI.copy.ME
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[IMWEB_PCI1.NT]         ; Win2k
 AddReg         = IMWEB_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = IMWEB_DRIVER.copy.NT, IMWEB_APPLET.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[IMWEB_PCI1.NT.5.1]         ; WinXP
 AddReg         = IMWEB_PCI1.reg, COMMON_PCI.reg.NT.5.1, COMMON_NDIS.reg.NT.5.1, COMMON.reg
 CopyFiles      = IMWEB_DRIVER.copy.NT.5.1, IMWEB_APPLET.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[IMWEB_PCI1.ME.Services]
 AddService     = "IMWEB", 2, IMWEB_DRIVER.Service, IMWEB_DRIVER.EventLog

[IMWEB_PCI1.ME.CoInstallers]
 CopyFiles      = IMWEB_COINSTALL.copy.NT
 AddReg         = IMWEB_COINSTALL.reg.NT

[IMWEB_PCI1.NT.Services]
 AddService     = "IMWEB", 2, IMWEB_DRIVER.Service, IMWEB_DRIVER.EventLog

[IMWEB_PCI1.NT.CoInstallers]
 CopyFiles      = IMWEB_COINSTALL.copy.NT
 AddReg         = IMWEB_COINSTALL.reg.NT

[IMWEB_PCI1.NT.5.1.Services]
 AddService     = "IMWEB51", 2, IMWEB_DRIVER.NT.5.1.Service, IMWEB_DRIVER.EventLog

[IMWEB_PCI1.NT.5.1.CoInstallers]
 CopyFiles      = IMWEB_COINSTALL.copy.NT
 AddReg         = IMWEB_COINSTALL.reg.NT

[IMWEB_PCI1.reg]
 HKR,Ndi        ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_25138086"
 HKR,           ,PlatformId,0,"0"
 HKR,           ,LoadFirmware,0,1
 ;HKR, NDI\params\LoadFirmware,,0,1

;============================================IMWEB_PCI2====================================================================
;[IMWEB_PCI2]            ; Win9x
; AddReg         = IMWEB_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
; CopyFiles      = IMWEB_DRIVER.copy, IMWEB_APPLET.copy, IMWEB_NDI.copy

;[IMWEB_PCI2.ME]         ; WinMe
; AddReg         = IMWEB_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
; CopyFiles      = IMWEB_DRIVER.copy.ME, IMWEB_APPLET.copy.ME, IMWEB_NDI.copy.ME
; BusType        = 5     ; PCI
; Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

;[IMWEB_PCI2.ME.ME]      ; WinMe - Same as .ME (Needed for Update Driver)
; AddReg         = IMWEB_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
; CopyFiles      = IMWEB_DRIVER.copy.ME, IMWEB_APPLET.copy.ME, IMWEB_NDI.copy.ME
; BusType        = 5     ; PCI
; Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

;[IMWEB_PCI2.NT]         ; Win2k
; AddReg         = IMWEB_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
; CopyFiles      = IMWEB_DRIVER.copy.NT, IMWEB_APPLET.copy.NT
; BusType        = 5     ; PCI
; Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

;[IMWEB_PCI2.NT.5.1]         ; WinXP
; AddReg         = IMWEB_PCI2.reg, COMMON_PCI.reg.NT.5.1, COMMON_NDIS.reg.NT, COMMON.reg
; CopyFiles      = IMWEB_DRIVER.copy.NT.5.1, IMWEB_APPLET.copy.NT
; BusType        = 5     ; PCI
; Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

;[IMWEB_PCI2.ME.Services]
; AddService     = "IMWEB", 2, IMWEB_DRIVER.Service, IMWEB_DRIVER.EventLog

;[IMWEB_PCI2.NT.Services]
; AddService     = "IMWEB", 2, IMWEB_DRIVER.Service, IMWEB_DRIVER.EventLog

;[IMWEB_PCI2.NT.5.1.Services]
; AddService     = "IMWEB51", 2, IMWEB_DRIVER.NT.5.1.Service, IMWEB_DRIVER.EventLog

;[IMWEB_PCI2.ME.CoInstallers]
; CopyFiles      = IMWEB_COINSTALL.copy.NT
; AddReg         = IMWEB_COINSTALL.reg.NT

;[IMWEB_PCI2.NT.CoInstallers]
; CopyFiles      = IMWEB_COINSTALL.copy.NT
; AddReg         = IMWEB_COINSTALL.reg.NT

;[IMWEB_PCI2.NT.5.1.CoInstallers]
; CopyFiles      = IMWEB_COINSTALL.copy.NT
; AddReg         = IMWEB_COINSTALL.reg.NT

;[IMWEB_PCI2.reg]
; HKR,Ndi        ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_25138086"
; HKR,           ,PlatformId,0,"0"
; HKR,           ,LoadFirmware,0,1
; HKR, NDI\params\LoadFirmware,,0,1
;=================================================================================================================

[IMWEB_COINSTALL.reg.NT]
 HKR,           ,CoInstallers32         ,0x00010000     ,"IMWEBCFG.cpl,NdiProc"

[IMWEB_DRIVER.Service]
 DisplayName    = %IMWEB_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\IMWEBN5.sys
 LoadOrderGroup = NDIS

[IMWEB_DRIVER.NT.5.1.Service]
 DisplayName    = %IMWEB_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\IMWEBN51.sys
 LoadOrderGroup = NDIS

[IMWEB_DRIVER.EventLog]
 AddReg         = IMWEB_DRIVER.EventLog.reg

[IMWEB_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

[IMWEB_DRIVER.ME.EventLog]
 AddReg         = IMWEB_DRIVER.ME.EventLog.reg

[IMWEB_DRIVER.ME.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_PCI.reg]
 HKR,NDI                ,Service                ,0      ,"IMWEB"
 HKR,NDI                ,CardType               ,0      ,"PCI"
 HKR,                   ,BusType                ,0      ,"5"
 HKR,                   ,DeviceVxDs             ,0      ,"IMWEBN5.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00

[COMMON_PCI.reg.NT.5.1]
 HKR,NDI                ,Service                ,0      ,"IMWEB51"
 HKR,NDI                ,CardType               ,0      ,"PCI"
 HKR,                   ,BusType                ,0      ,"5"
 HKR,                   ,DeviceVxDs             ,0      ,"IMWEBN51.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00

[COMMON_NDIS.reg]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI                ,NdiInstaller           ,0      ,"IMWEBCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"IMWEB"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a


 HKR,defaults,PSMode,0,1
 ;HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,1,0

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI                ,NdiInstaller           ,0      ,"IMWEBCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"IMWEB"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a


 HKR,defaults,PSMode,0,1
 ;HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,1,0



[COMMON_NDIS.reg.NT]
 HKR,                   ,EnumPropPages32        ,0      ,"IMWEBCFG.cpl,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

 HKR,defaults,PSMode,0,1
 ;HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,1,0


[COMMON_NDIS.reg.NT.5.1]
 HKR,                   ,EnumPropPages32        ,0      ,"IMWEBCFG.cpl,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

 HKR,defaults,PSMode,0,1
 ;HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
 HKR,NDI\params\PSMode,optional,1,0

[COMMON.reg]

 HKR,                   ,IMWEBIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,defaults,LoadFirmware,0,1
;HKR,NDI\params\LoadFirmware,,0,1 
 HKR,Ndi\params\LoadFirmware,default,0,1
 HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
 HKR,NDI\params\LoadFirmware,type,,enum
 HKR,NDI\params\LoadFirmware,flag,1,30,00,00,00
 HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
 HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
 HKR,NDI\params\LoadFirmware,optional,1,0

 HKR,defaults,ListenInterval,0,3
; HKR,NDI\params\ListenInterval,,0,3
 HKR,Ndi\params\ListenInterval,default,0,3
 HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
 HKR,NDI\params\ListenInterval,type,,int
 HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
 HKR,NDI\params\ListenInterval,min,0,0
 HKR,NDI\params\ListenInterval,max,0,77
 HKR,NDI\params\ListenInterval,step,0,1
 HKR,NDI\params\ListenInterval,optional,1,0

 HKR,defaults,RTSThresh,0,2432
 ;HKR,NDI\params\RTSThresh,,0,2432
 HKR,Ndi\params\RTSThresh,default,0,2432
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2432
 HKR,NDI\params\RTSThresh,step,0,64
 HKR,NDI\params\RTSThresh,optional,1,0

 HKR,defaults,FragThresh,0,2432
; HKR,NDI\params\FragThresh,,0,2432
 HKR,Ndi\params\FragThresh,default,0,2432
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2432
 HKR,NDI\params\FragThresh,step,0,128
 HKR,NDI\params\FragThresh,optional,1,0

 HKR,defaults,PreambleMode,0,3
; HKR,NDI\params\PreambleMode,,0,1
 HKR,Ndi\params\PreambleMode,default,0,3
 HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
 HKR,NDI\params\PreambleMode,type,,enum
 HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
 HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
 HKR,NDI\params\PreambleMode,optional,1,0

 HKR,defaults,AuthentAlg,0,65535
; HKR,NDI\params\AuthentAlg,,0,65535
 HKR,NDI\params\AuthentAlg,default,0,65535
 HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
 HKR,NDI\params\AuthentAlg,type,,enum
 HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
 HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
 HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
 HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
 HKR,NDI\params\AuthentAlg,optional,1,0

 HKR,defaults,AdhocDemoMode,0,0
; HKR,NDI\params\AdhocDemoMode,,0,0
 HKR,Ndi\params\AdhocDemoMode,default,0,0
 HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
 HKR,NDI\params\AdhocDemoMode,type,,enum
 HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
 HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
 HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
 HKR,NDI\params\AdhocDemoMode,optional,1,0

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;NOTE: This section (Intersil Method) is commented out due to
;IBM request for modification in PDwellTime interface
; 
; HKR,defaults,PDwellTime,0,120
; HKR,NDI\params\PDwellTime,,0,120
; HKR,Ndi\params\PDwellTime,default,0,120
; HKR,NDI\params\PDwellTime,ParamDesc,0,%PDWELL_STR%
; HKR,NDI\params\PDwellTime,type,0,int
; HKR,NDI\params\PDwellTime,flag,1,20,00,00,00
; HKR,NDI\params\PDwellTime,min,0,0
; HKR,NDI\params\PDwellTime,max,0,1000
; HKR,NDI\params\PDwellTime,step,0,1
; HKR,NDI\params\PDwellTime,optional,0,1
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

 HKR,defaults,PDwellTime,0,0
; HKR,NDI\params\PDwellTime,,0,0
 HKR,Ndi\params\PDwellTime,default,0,0
 HKR,NDI\params\PDwellTime,ParamDesc,0,%EXTENDED_CHANNEL_MODE_STR%
 HKR,NDI\params\PDwellTime,type,0,enum
 HKR,NDI\params\PDwellTime,flag,1,30,00,00,00
 HKR,NDI\params\PDwellTime\enum,0,,"Disable (For N. America)"
 HKR,NDI\params\PDwellTime\enum,100,,"Enable"
 HKR,NDI\params\PDwellTime,optional,1,0


 HKR,defaults,11dMode,0,0
; HKR,NDI\params\11dMode,,0,0
 HKR,Ndi\params\11dMode,default,0,0
 HKR,NDI\params\11dMode,ParamDesc,,%MDC_CONTROL_STR%
 HKR,NDI\params\11dMode,type,,enum
 HKR,NDI\params\11dMode,flag,1,30,00,00,00
 HKR,NDI\params\11dMode\enum,0,,"None"
 HKR,NDI\params\11dMode\enum,1,,"Strict"
 HKR,NDI\params\11dMode\enum,2,,"Flexible"
 HKR,NDI\params\11dMode,optional,1,0

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir                 = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 IMWEB_DRIVER.copy              = 11 ; Win9x=%windir%\system
 IMWEB_DRIVER.copy.ME           = 11 ; Win9x=%windir%\system
 IMWEB_DRIVER.copy.NT           = 12 ; Win2k=%windir%\system32\drivers
 IMWEB_DRIVER.copy.NT.5.1       = 12 ; WinXP=%windir%\system32\drivers

[IMWEB_NDI.copy]
 IMWEBR16.dll           ; Win9x NDI
 IMWEBCFG.dll           ; Win9x NDI

[IMWEB_NDI.copy.ME]
 IMWEBR16.dll           ; Win9x NDI
 IMWEBCFG.dll           ; Win9x NDI

[IMWEB_COINSTALL.copy.ME]
 IMWEBRES.dll
 IMWEBIOC.dll
 IMWEBCFG.cpl           ; Win2k CoInstaller

[IMWEB_COINSTALL.copy.NT]
 IMWEBRES.dll
 IMWEBIOC.dll
 IMWEBCFG.cpl           ; Win2k CoInstaller

[IMWEB_DRIVER.copy]
 IMWEBN5.sys
 IMWEBIOC.vxd           ; Win9x Ioctl interface

[IMWEB_DRIVER.copy.ME]
 IMWEBN5.sys
 IMWEBIOC.vxd           ; Win9x Ioctl interface

[IMWEB_DRIVER.copy.NT]
 IMWEBN5.sys

[IMWEB_DRIVER.copy.NT.5.1]
 IMWEBN51.sys

[IMWEB_APPLET.copy]
 IMWEBRES.dll
 IMWEBIOC.dll
 IMWEBCFG.cpl
 IMWEBSTA.exe

[IMWEB_APPLET.copy.ME]
 IMWEBRES.dll
 IMWEBIOC.dll
 IMWEBCFG.cpl
 IMWEBSTA.exe

[IMWEB_APPLET.copy.NT]
;IMWEBRES.dll           ; Copied by coinstaller
;IMWEBIOC.dll           ; Copied by coinstaller
;IMWEBCFG.cpl           ; Copied by coinstaller
;IMWEBCFG.hlp           ; Copied by coinstaller
;IMWEBCSH.dll           ; Copied by coinstaller
 IMWEBSTA.exe

[SourceDisksNames]
1 = %INSTALL_DISK_STR%,,,


[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
IMWEBR16.dll           = 1,win9x
IMWEBCFG.dll           = 1,win9x
IMWEBIOC.vxd           = 1,win9x
IMWEBIOC.dll           = 1
IMWEBCFG.cpl           = 1,winnt
IMWEBSTA.exe           = 1
IMWEBRES.dll           = 1
IMWEBN5.sys            = 1
IMWEBN51.sys	       = 1,WinXP

[SourceDisksFiles.ME]   ; WinMe
IMWEBR16.dll           = 1,win9x
IMWEBCFG.dll           = 1,win9x
IMWEBIOC.vxd           = 1,win9x
IMWEBIOC.dll           = 1
IMWEBCFG.cpl           = 1,winnt
IMWEBN5.sys            = 1
IMWEBSTA.exe           = 1

[SourceDisksFiles.X86]  ; Win2k
IMWEBRES.dll           = 1
IMWEBIOC.dll           = 1
IMWEBCFG.cpl           = 1,Win2k
IMWEBN5.sys            = 1
IMWEBSTA.exe           = 1

[SourceDisksFiles.NT.5.1]  ; WinXP
IMWEBRES.dll           = 1
IMWEBIOC.dll           = 1
IMWEBCFG.cpl           = 1,Win2K
IMWEBN51.sys           = 1,WinXP
IMWEBSTA.exe           = 1


;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         	= "Intel"
 VER_VENDOR_NAME_STR    	= "Intel Corporation"
 IMWEB_PCI1_STR         	= "High Rate Wireless LAN Mini-PCI Adapter with Modem II"
;IMWEB_PCI2_STR         	= "High Rate Wireless LAN Mini-PCI Adapter with Modem II"
 IMWEB_SERVICE_DISPLAY  	= "High Rate Wireless LAN Mini-PCI LAN Driver"
 INSTALL_DISK_STR       	= "High Rate Wireless LAN Mini-PCI Install Disk"
 ADHOC_DEMO_STR         	= "Adhoc Demo Mode"
 SHORT_PREAM_STR        	= "Preamble Mode"
 RTSTHRESH_STR          	= "RTS Threshold"
 FRAGTHRESH_STR         	= "Fragmentation Threshold"
 AUTHENT_TYPE_STR       	= "Authentication Algorithm"
 LISTENINTERVAL_STR     	= "Listen Interval"
 POWER_SAVE_STR         	= "Power Save Mode"
 POWER_LEVEL_STR        	= "Power Save Level"
 PDWELL_STR            		= "Passive Scan Dwell"
 LOAD_FIRMWARE_STR      	= "Firmware Download"
 EXTENDED_CHANNEL_MODE_STR	= "Extended Channel Mode"
 MDC_CONTROL_STR        	= "802.11D Control"