### Unite Storager**

The SOM-based Unite Storager provides native OS/2 device driver support for a variety of SCSI-based storage devices and a complete set of APIs to store and retrieve data from optical and CD-recordable media within a jukebox. A graphical user interface is provided to start, control, tune, and stop Unite Storager; and administrative functions such as the importing, labeling, and exporting of platters can be performed using this interface. Dynamic, user-defined tuning parameters are available for optimizing performance. Data is stored to the media either in high-performance data blocks or standard FAT file system approach.

### Multi-Threaded Performance

Unite Storager takes full advantage of OS/2's multi-tasking capabilities to manage thousands of store and retrieve requests while simultaneously reading and writing to all drives in the jukebox. Unite Storager's multi-threaded design is so efficient, it can even burn CD-recordable discs while under the heaviest retrieval loads. There's no need to schedule CD-R burns for the middle of the night.

### Optimization of Storage Management Requests

Store and retrieve requests are sorted by type and volume name to maximize throughput and minimize retrieval wait time. Your data will be retrieved quickly, no matter how heavy the storage load.

### Automatic CD-ROM Duplication

With a flip of a check box, Unite Storager can be instructed to create a second copy of each CD-ROM burned. The duplicate CD-ROMs can then be removed and stored elsewhere for maximum backup protection.

For more information, please contact:

| Cirrus Technology, Inc. 5301 Buckeystown Pike, Fourth Floor Frederick, MD 21704 Phone: 1-301-698-1900 FAX: 1-301-698-1909
E-mail: sales@cirunite.com
CompuServe: GO UNITE
Web: www.cirunite.com

[ Catalog Home ]