MUST BE IN DOS ON BOOTUP
CAN NOT FLASH WITHIN ANY OPERATING SYSTEM

RUN AMIFLASH.COM FROM FLOPPY OR HARD DRIVE BY TYPING


WHEN PROMPTED TO 		ENTER

"SAVE EXISTING ROM" 		"Y" OR "N"

"ENTER BIOS FILENAME"		PATH OF FILE, EXAMPLE (C:\ROMFILE.ROM)   
  
"PROGRAM BOOTBLOCK"  		"Y"  (YOU MUST SELECT Y)

"PRESS Y TO CONTINUE"		"Y"


AMIFLASH WILL THEN PROCEED TO UPDATE THE FLASH PART.
AFTER SUCCESSFUL COMPLETION, PRESS ANY KEY TO RESTART.


IMPORTANT NOTE

IF YOU HAVE A MESSAGE THAT CAN NOT FIND FLASH ROM 
HIT THE CTRL+ALT+DELETE TO RESTART YOUR COMPUTER FOR
A SOFT RESET THEN CONTINUE WITH AMIFLASH PROGRAM.

IMPORTANT NOTE

WHEN RUNNING AMIFLASH.COM DO NOT ADD ROMFILE NAME IN RUNNING PROGRAM.
JUST RUN AMIFLASH.COM AND ENTER ROMFILE NAME DURING SETUP OF THE BIOS UPGRADE.



