# FreeBSD notes

WorkMan was ported to FreeBSD by Todd Pfaff (todd@flex.eng.mcmaster.ca).

This port was developed and tested on the following:

- FreeBSD-1.1-BETA
- XFree86-2.0
- xview3.2 (from the FreeBSD ports collection)
- Adaptec 1542C SCSI controller
- Toshiba XM-3401B CDROM drive

## Building from source

If you have FreeBSD-1.1, XFree86-2.0 and xview3.2 installed you should be able to build and install workman with:

> xmkmf
> make
> make install
> make install.man

## Known problems

All CD drive IO is done using the FreeBSD CDIO interface defined in cdio.h. I didn't attempt to write the wm_scsi() SCSI interface code in plat_freebsd.c so direct SCSI support is not available. Implementing this would allow the SCSI drive specific routines from drv_*.c to be taken advantage of. Perhaps the SCSI user library submitted to the FreeBSD-hackers list by Peter Dufault (hd@world.std.com) could be used for this purpose.

The CDIOREADTOCENTRYS fails if an attempt is made to read past the last track found with CDIOREADTOCHEADER and I couldn't figure out any way to get the length of the last CD track. If anyone fixes this please let me know how. I hardcoded the last track length as 10 minutes which is obviously an ugly solution.

The CDIOCEJECT ioctl doesn't eject the CD from my drive.

The volume control isn't the greatest and I didn't spend any time trying to improve it.

The balance control doesn't work very well.

To the install page

##### Last update: 02 Jun 1995