Documentation on Command Line Switches is Incorrect

Product Version(s): 3.20
Operating System:   MS-DOS
Flags: ENDUSER | docerr
Last Modified: 18-AUG-1988    ArticleIdent: Q10285

Question:
   Concerning Table 18.6, "Command Line Switches" on Page 347 of the
"Microsoft Pascal Reference" manual for Version 3.20, and Table 5.2,
"Pass One Compiler Switches," on Page 51 of the "Microsoft Pascal
Compiler User's Guide;" which one of the two lists is correct?
   Concerning the switch /L; does this refer to the SYMDEB debugger
that comes with Microsoft Macro Assembler, or the DOS Debug?

Response:
   Table 18.6, on Page 347 of the Pascal reference manual is
correct.
   The debugger is SYMDEB. Debug does not detect line numbers.
