Knowledge Base |

# HP JetDirect Firmware Versions and Windows NT Protocol Support

Article ID: 124293

Article Last Modified on 11/1/2006

APPLIES TO

- Microsoft Windows NT Workstation 3.5
- Microsoft Windows NT Workstation 3.51
- Microsoft Windows NT Workstation 4.0 Developer Edition
- Microsoft Windows NT Server 3.5
- Microsoft Windows NT Server 3.51
- Microsoft Windows NT Server 4.0 Standard Edition

This article was previously published under Q124293
Windows NT can print to most Hewlett-Packard (HP) JetDirect network printer cards using either the data link control (DLC) protocol or the TCP/IP protocol using Line Printer Remote (LPR)/Line Printer Daemon (LPD). However, not all JetDirect cards support all protocols. The firmware revision of a JetDirect card determines its ability to work with Windows NT network printing protocols.
The following list outlines the Windows NT protocols and capabilities supported by the different HP JetDirect firmware revisions.

    Version         Description
    --------        -----------------------------------------------------------

    A.03.03         Fully supports LPD for TCP/IP printing and DLC with
    or later        automatic protocol switching in any HP printer that
                    supports the card.

    A.03.00 -       Fully supports DLC with protocol switching in any HP
      A.03.02       printer that supports the card. This firmware
                    revision does not support LPD. Therefore, even though it
                    does support TCP/IP, it does not work with the Windows NT
                    LPR TCP/IP printing client.

    A.02.0x         Supports DLC, but can only use protocol switching on
                    an HP 4Si. If you are using another printer, the other
                    protocols must be disabled for Windows NT DLC to work
                    properly. This firmware revision does not support LPD.
                    Therefore, even though it does support TCP/IP, it will not
                    work with Windows NT's LPR TCP/IP printing client.

    A.01.0x         Supports DLC, but all other protocols must be disabled.
                    There is no protocol switching support with this firmware
                    revision on any HP printer.

A.00.0x No DLC support, will not work with Windows NT.
The firmware revision of an HP JetDirect card can normally be found by printing the printer self-test page on a printer with the card installed. The revision number is preceded by:

       FIRMWARE REVISION:

For additional information, contact Hewlett-Packard Technical Support at (208) 323-2551.
The HP JetDirect network printer card is manufactured by Hewlett-Packard Company, a vendor independent of Microsoft; we make no warranty, implied or otherwise, regarding this products' performance or reliability.

Additional query words: prodnt tcpip

Keywords: kbprint KB124293