Knowledge Base |

# MemMaker .STS Err Msg (Adaptec 1742A SCSI / ASPIEDOS.SYS)

Article ID: 106229

Article Last Modified on 11/22/1999

APPLIES TO

- Microsoft MS-DOS 6.2 Standard Edition
- Microsoft MS-DOS 6.21 Standard Edition
- Microsoft MS-DOS 6.22 Standard Edition

This article was previously published under Q106229

## SYMPTOMS

If you have an Adaptec 1742A SCSI card, you may receive an error message indicating the MEMMAKER.STS file has been corrupted when you run MS-DOS MemMaker.

## CAUSE

This problem occurs when MemMaker tries to determine the size of the ASPIEDOS.SYS device driver.

## RESOLUTION

To work around this problem, edit the MEMMAKER.INF file and add the following lines:

       ^ASPIEDOS

Additional query words: 6.22 6.20 ^ASPI2DOS ^ASPICD 2940 series 1540

Keywords: KB106229