Knowledge Base |

# Compaq Netflex Doesn't Recover from Network Cabling Removal

Article ID: 103025

Article Last Modified on 4/8/2004

APPLIES TO

- Microsoft Windows NT Advanced Server 3.1
- Microsoft Windows NT Workstation 3.1
- Microsoft Windows NT Advanced Server 3.1

This article was previously published under Q103025

## SUMMARY

Compaq Netflex network adapters, in token ring mode, fail to recover if you remove and put back the network cabling. This problem is caused by the device driver.

Additional query words: prodnt

Keywords: kbhardware KB103025