Knowledge Base |

# TCP/IP Stack for Workgroups Add-On 3.11 Fails to Load

PSS ID Number: 115835

Article Last Modified on 12/10/2000

The information in this article applies to:

- Microsoft Workgroup Add-On for MS-DOS 3.11

This article was previously published under Q115835

## SYMPTOMS

The setup procedure of the TCP/IP stack for Windows for Workgroups 3.11 to Workgroups Add-On version 3.11 does not prompt for the default gateway, IP address, and Subnet mask. As a result, TCP/IP stack fails to load.

## RESOLUTION

After setup of TCP/IP is complete, do the following:

1. Add the following three lines to the [TCPIP] section of the PROTOCOL.INI file:

          DefaultGateway0= <default gateway address>
          SubnetMask0= <subnet mask>
          IPAddress0= <IP address>

   NOTE: Each octet above must be separated by a space.
2. Save the PROTOCOL.INI file and reboot the workstation.

Additional query words: wfw wfwg 3.11

Keywords: KB115835
Technology: kbAudDeveloper kbWFW311DOS kbWFWSearch