Knowledge Base |

# MS2000$ Trap D on OS/2 2.1 Workstation

Article ID: 108487

Article Last Modified on 10/31/2006

This article was previously published under Q108487

## SYMPTOMS

The Microsoft LAN Manager NE2000 driver MS2000.OS2 dated 6/23/93 causes a Trap d when booting on an OS/2 2.1 workstation.

## WORKAROUND

Currently the only workaround is to change network interface cards or use OS/2 2.0.

## STATUS

Microsoft has confirmed this to be a problem in LAN Manager NE2000 driver MS2000.OS2. We are researching this problem and will post new information here in the Microsoft Knowledge Base as it becomes available.

## MORE INFORMATION

Exception in device driver: MS2000$
TRAP 000D ERRACD=0008 ERRAC=**** ERLIM=********
EAX=0000000 EBX=7BCC0828 EXC=0001-860 EDX=00000008
ESI=3BDC021E EDI=FCA90174 EBP=00004CC0 FLG=00013206
CS:ELP=0820:0000051A CSACC=0096 CSLIM=00002854
SS:ESP=0030:00004CBA SSAC=1097 SSLIM=00003FFF
DS=0818 DSACC=0093 DSLIM=000021AC CR0=FFFFFFFB
ES=0818 ESALL=0093 ESLIM=000021AC CR2=1A055354
FS=0000 FASALL=**** FSLIM=********
GS=0000 GSALL=**** GSLIM=********
The system detected an internal processing error at location ##0160:fff5fbd5-000d:9bd5
038600d1
Internal revision 6.514, 93/04/12
The System stopped.

Additional query words: 2.20 2.2

Keywords: KB108487