Cannot Print to Bin 2 on the Canon BJ-300 or BJ-330 Printer
  
PSS ID Number: Q102656
Article last modified on 11-03-1994
 

 

 

======================================================================
6.00
MS-DOS
kbother
 
-------------------------------------------------------------------
The information in this article applies to:
 
 - Microsoft Word for MS-DOS, version 6.0
-------------------------------------------------------------------
 
You cannot print to Bin 2 on the Canon BJ-330 (Sheetfeeder) or BJ-300
(Sheetfeeder) printers by selecting Bin 2 from the Paper Feed list in
the Printer Setup dialog box in Word for MS-DOS. This setting has no
effect on bin selection for either printer. You must select the bin
using the printer control panel.
 
The default bin selection on the Canon BJ-330/300 printers is Bin 1.
To select Bin 2 as the paper feed source, press the Paper button on
the printer control panel.
 
There is no escape sequence to control bin selection on the Canon
BJ-300 or BJ-330 printers, so you cannot select Bin 2 by embedding a
printer escape code in your Word document.
 
The products included here are manufactured by Canon, a vendor
independent of Microsoft; we make no warranty, implied or otherwise,
regarding these products' performance or reliability.
 
REFERENCES
==========
 
"Canon BJ-300/330 User's Manual," page III-16
 
"Canon BJ-300/330 Programmer's Manual"
 
KBCategory: kbother
KBSubcategory:
Additional reference words: 6.00
======================================================================
=============================================================================
Copyright Microsoft Corporation 1994.