## Reports Task Flow

Task | Description | For Instructions
--- | --- | ---
Revision Reports Tasks
Start revision checking on specific product categories. | Revision Checking checks the software, hardware, and firmware revisions of all the user-selected components. Revision checking is based on an updatable matrix, which is generated using the PatchPro database. | Run Report
Check software revision levels | The Display Report page enables you to check software revision levels and save the Revision Checking Report to the archive database. | Display Report
Review archived revision checking reports. | The Display History window enables you to review archived revision checking reports. | Display History
Reports Administration Tasks
Displaying a summary of the device Customizing the FRU report using a filter | Using the FRU report, you can quickly display a summary of the status of your device and further customize the report using the filters provided. | FRU Reports
Displaying archived FRU reports | Displays archived FRU reports. | FRU Report History
Displaying a summary of Sun StorEdge 6120 array exceptions | Using the Exception report, you can quickly display a summary of the status of the Sun StorEdge 6120 array exceptions, which are defined in System/exception.conf | Exception Report
Displaying a summary of the events relating to a device Customizing an event report using filters | Using the Event report, you can quickly display a summary of the status of your device and further customize the report using the filters provided. | Event Statistics
Displaying all devices with health and alert information | The Device Health Summary displays all devices with health and alert information.It summarizes the information from the FRU Report and Event Report. | Device Summary
Setting up Report Scheduler to email reports on a regular basis | The Report Scheduler can be used to email reports on a regular basis. | Report Scheduler
Checking Agent Statistics | Agent execution statistics | Agent Statistics
Clearing a specified number of maximum email messages | The Email and Events Maximums page displays the output of the database that keeps track of the number of events and email messages that are sent per device or component. | Email and Event Maximums
Displaying the Thresholds | The Thresholds window displays the thresholds that are used to monitor entries related to I/O interfaces in the /var/adm/messages file. | Thresholds List
Reviewing switch data | Use the Switch Data functionality to view the values of Fibre Channel counters in a report format. After you have set the Set-Baseline field, the Switch Data report displays counter increments, sorted by component, and the start time and duration of the set baseline. | Switch Data
Displaying device attributes Displaying event severity | The Event and Severity Mapping report displays every device attribute the agents search for when monitoring the devices. In addition, this report displays the severity for each event and whether or not the event is actionable. | Event and Severity Mapping

##