## Device Discovery Page

Field | Description
Agents running | Displays how many agents are currently running.
Agents done | Displays how many agents have completed the discovery run.
Devices found | Click to display details about the discovered devices in a pop-up window. The results show the following: Agent Type-device type Name IP-IP address of the device Comments
Host | Select a host from the pull-down menu from which the agents will run.
Product/Discovery Method | Select a product or a discovery method from the following list: Devices from IP List (the default)-All devices that have been entered in the `/etc/deviceIP.conf` file are discovered. Depending on the size of the monitored configuration, this process might take a few minutes. Note: JOBOD devices cannot be discovered using the Devices from IP List method. Inband discovery-In-band devices, including internal disks, Sun StorEdge A5x00 arrays, and tape devices are discovered. Inband Sun 3120JBOD/3310JBOD/3310/3510/3511 Discovery - Includes: StorEdge 3120 SCSI array (JBOD) Sun StorEdge 3310 SCSI array (RAID Controller) Sun StorEdge 3310-D SCSI array (JBOD) Sun StorEdge 3510 FC array (RAID Controller) Sun StorEdge 3511 FC array (RAID-SATA Controller) Sun StorEdge A3500FC array Sun StorEdge D2 array Subnet-uses SNMP to query and discover supported switches and arrays. Sun StorEdge systems, such as the Sun StorEdge 6320 and 6920 system, can be discovered using either Devices from IP List or Subnet.
| Click to activate Discovery.