## Discovery

All monitored devices can be individually selected from the Product/Discovery Method menu. The default is Devices from IP List, meaning all devices that have been entered in the `/etc/deviceIP.conf` file are discovered.

Depending on the size of the monitored configuration, this process might take a few minutes.

The Subnet discovery method uses SNMP to query and discover supported switches and arrays. Sun StorEdge systems, such as the Sun StorEdge 6320 and 6920 system, can be discovered from either Devices from IP List or from the Subnet.

Note -

Discovery methods marked background indicate that, because the discovery is running in the background, the user can continue on to another task.