## Manually Updating a Device

1. Click the Maintain Devices link from the General Maintenance menu.

The Maintain Devices window is displayed.

Note -

The IP Address is a unique number that identifies the device. The worldwide name and Key number are unique identifiers for a specific FRU. Although none of the identifiers are user-maintainable, they help Sun service representatives troubleshoot by enabling them to track the FRUs to specific Sun StorEdge 6120 arrays.

2. Select the device you want to update from the Device Name column.
3. Correct the necessary fields and click Update.

Note -

Changing the name of the device changes only the reference to that device within the Storage Automated Diagnostic Environment. It does not affect the access or reference to that device within the operating system.

Note -

If you change the configuration of a device, you must delete that unwanted device, using the functionality described in Deleting a Device.
The Storage Automated Diagnostic Environment topology does not display a device until you manually add and discover the device using the functionality described in Maintaining Devices.

### Related Topics

- Update Device Page