## Switch Data Page

Field | Description
--- | ---
Select Switch | The switch type pull-down menu, from which you can select a switch about which Fibre Channel counters are displayed.
Display | Click Display to activate the Select Switch feature, after the switch has been selected.
Set-Baseline | The Switch Data report displays the starting date, time, and duration of the baseline. Any increase of Fibre Channel counters after the baseline is set is displayed in bold (for example, 10/100).
Total | Click Total to erase the values saved by Set-Baseline and to display the total Fibre Channel counters (the actual values)