## SNMP Trap Provider Page

Function | Description
Active | Select to activate the provider. Deselect to make the provider inactive.
SNMP Version | Select version number; `v1` is the default.
IP Name/Address | Type the IP name and address that identifies the host to the network. You can provide information for up to five IP addresses.
Port | Specify the port number; default is 162.
Min Alert Level | Warning is the default. Warning-yellow Error-red Down-red