## Retrieving Tokens From an Array

This command changes the configuration of all Sun StorEdge 6120 arrays that are components of a Sun StorEdge Solution system.

1. Click Run Scripts in the System Utilities window.

The Run Scripts window is displayed.

1. Click the Retrieve Tokens From an Array script from the script list.
2. Type the IP address of the Sun StorEdge 6120 array in the IP text box.
3. `0` or `1`: Select a `0` or `1` for the first or second enclosure (in an HA configuration).
4. Select type of data: `elemprop`, `sysprop`, `systemfru`, `frudata`, `fruprop`, `portprop`, `slice`, `volprop`, `vol`, `lun`, `loopin`, `sysdata`.
5. Click Run Command.