## Local Notification (Email/Scripts)

You can use the Local Email/Pager Notifications window to customize the generation of email messages to yourself or to other administrators at their companies. For example, if you are interested in receiving only high-priority alerts coming from Sun StorEdge 6120 arrays, you can create a specialized notification for this instance only.

Note -

Alerts are sent only to valid email addresses that you have entered through the Email Notification function. Local notification does not send mail to the email provider.

In addition to sending the RAS information collected by the Storage Automated Diagnostic Environment, you can send a customized subset of the event-driven messages from the host directly to local system administrators at the customer's site by email.

For events that produce frequent error messages, you can specify the number of times you are notified. If the maximum number is set to a value other than "no maximum" (the default), you can receive an email 5, 10, 20, or 50 times within an eight-hour period. The last email message indicates that it is the final notification you will receive within the eight-hour time period.

Note -

If you have set the maximum number of email messages to 6, have received 6 messages on the same component within an eight-hour time period, and want to receive more email notifications, you must click the Clear Email maximums button.