Patch-ID# 117350-05
Platform: Fujitsu PRIMEPOWER(GP7000F)

Relevant Architectures: sparc.sun4us

Date:   2004.06.21.10.55

Special Note:

	To get the complete fix for 4860955 and 4893666 for 
	PRIMEPOWER 900/1500/2500 systems with FJSV,SPARC64-V processors,
	one needs to install the following patch:

	111789-06 (or newer)	/platform/SUNW,Ultra-Enterprise-10000/
				kernel/drv/dr patch

	To confirm that the system is a PRIMEPOWER 900/1500/2500 systems
	with FJSV,SPARC64-V processors, verify that the "uname -i" 
	command returns "FJSV,GPUZC-L".

	example# uname -i
	FJSV,GPUZC-L

Patches which conflict with this patch:

Patches required with this patch: 108528-29 117000-05 (or newer)

Files included with this patch:

	/kernel/drv/sparcv9/log
	/platform/FJSV,GPUSC-L/kernel/cpu/FJSV,SPARC64-IV
	/platform/FJSV,GPUSC-L/kernel/cpu/sparcv9/FJSV,SPARC64-IV
	/platform/FJSV,GPUSC-L/kernel/genunix
	/platform/FJSV,GPUSC-L/kernel/sparcv9/genunix
	/platform/FJSV,GPUSC-L/kernel/sparcv9/unix
	/platform/FJSV,GPUSC-L/kernel/unix
	/platform/FJSV,GPUSC-M/kernel/cpu/FJSV,SPARC64-IV
	/platform/FJSV,GPUSC-M/kernel/cpu/sparcv9/FJSV,SPARC64-IV
	/platform/FJSV,GPUSC-M/kernel/genunix
	/platform/FJSV,GPUSC-M/kernel/sparcv9/genunix
	/platform/FJSV,GPUSC-M/kernel/sparcv9/unix
	/platform/FJSV,GPUSC-M/kernel/unix
	/platform/FJSV,GPUSK/kernel/cpu/FJSV,SPARC64-III
	/platform/FJSV,GPUSK/kernel/cpu/FJSV,SPARC64-IV
	/platform/FJSV,GPUSK/kernel/cpu/sparcv9/FJSV,SPARC64-III
	/platform/FJSV,GPUSK/kernel/cpu/sparcv9/FJSV,SPARC64-IV
	/platform/FJSV,GPUSK/kernel/genunix
	/platform/FJSV,GPUSK/kernel/sparcv9/genunix
	/platform/FJSV,GPUSK/kernel/sparcv9/unix
	/platform/FJSV,GPUSK/kernel/unix
	/platform/FJSV,GPUZC-L/kernel/cpu/FJSV,SPARC64-V
	/platform/FJSV,GPUZC-L/kernel/cpu/sparcv9/FJSV,SPARC64-V
	/platform/FJSV,GPUZC-L/kernel/genunix
	/platform/FJSV,GPUZC-L/kernel/sparcv9/genunix
	/platform/FJSV,GPUZC-L/kernel/sparcv9/unix
	/platform/FJSV,GPUZC-L/kernel/unix
	/platform/FJSV,GPUZC-M/kernel/cpu/FJSV,SPARC64-V
	/platform/FJSV,GPUZC-M/kernel/cpu/sparcv9/FJSV,SPARC64-V
	/platform/FJSV,GPUZC-M/kernel/genunix
	/platform/FJSV,GPUZC-M/kernel/sparcv9/genunix
	/platform/FJSV,GPUZC-M/kernel/sparcv9/unix
	/platform/FJSV,GPUZC-M/kernel/unix
	/platform/sun4us/kernel/cpu/FJSV,SPARC64-III
	/platform/sun4us/kernel/cpu/FJSV,SPARC64-IV
	/platform/sun4us/kernel/cpu/sparcv9/FJSV,SPARC64-III
	/platform/sun4us/kernel/cpu/sparcv9/FJSV,SPARC64-IV
	/platform/sun4us/kernel/genunix
	/platform/sun4us/kernel/sparcv9/genunix
	/platform/sun4us/kernel/sparcv9/unix
	/platform/sun4us/kernel/unix
	/usr/platform/sun4us/include/sys/spitregs.h

Problem Description:

(from 117350-03)
	UC#2108 Memscrubber needs to be aware of retired pages.
	UC#2121 Enabling automatic cpu removal for Fujitsu platforms.

(from 117350-01)
	UC#2102 SPARC64-V systems may miss cache way degradation event.

	Please refer to patch README file.

