Patch-ID# 108839-03
Keywords: security deallocate list_devices mkdevamaps mkdevalloc
Synopsis: SunOS 5.7_x86: allocate/mkdevmaps/mkdevalloc Patch
Date: Nov/13/2001

Solaris Release: 7_x86

SunOS Release: 5.7_x86

Unbundled Product: 

Unbundled Release: 

Xref: This patch available for SPARC as patch 108838

Topic: SunOS 5.7_x86: allocate/mkdevmaps/mkdevalloc patch
       NOTE:  Refer to Special Install Instructions section for 
              IMPORTANT specific information on this patch.

Relevant Architectures: i386

BugId's fixed with this patch: 1229659 4223467 4284187 4316613

Changes incorporated in this version: 1229659 4284187

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/usr/sbin/allocate
/usr/sbin/deallocate
/usr/sbin/list_devices
/usr/sbin/mkdevalloc
/usr/sbin/mkdevmaps

Problem Description:

1229659 mkdevalloc & mkdevmap spin/core dump on Solaris Base Server
4284187 mkdevmaps generates bad entry for fd0 on x86
 
(from 108839-02)
 
4316613 mkdevmaps lists devices for sr0 as c0t0d0s0 instead of c1t6d0s0
 
(from 108839-01)
 
4223467 allocate broken in Solaris 7
4284187 mkdevmaps generates bad entry for fd0 on x86

Patch Installation Instructions:
--------------------------------
 
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-8 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
       example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
       example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
----------------------------- 
 
	NOTE : 	If BSM has already been activated, the file,
	        /etc/security/device_allocate, should be inspected 
	        for corrupted entries.  These will show up with the 
	        vi editor as non-ascii characters. If a bad entry
                is found, then the mkdevalloc program should be run
	        (as the root user) and the device_allocate file
	        regenerated.
 
	        	mkdevalloc > device_allocate.new
 
	        Compare old and new versions of device_allocate to 
		verify correct entries. Replace device_allocate with
                new version.

README -- Last modified date:  Tuesday, November 13, 2001

