Patch-ID# 142704-01

NOTE:
***********************************************************************
READ THE TERMS OF THE AGREEMENT ("AGREEMENT") IN THE LEGAL_LICENSE.TXT
FILE CAREFULLY BEFORE USING THIS SOFTWARE. BY USING THE SOFTWARE, YOU
AGREE TO THE TERMS OF THIS AGREEMENT. IF YOU DO NOT AGREE TO ALL OF THE
TERMS, PROMPTLY DESTROY THE UNUSED SOFTWARE.
***********************************************************************
For further information on patching best practices and resources, please
see the Big Admin Patching Center, http://www.sun.com/bigadmin/patches/ 
***********************************************************************

Keywords: sun ultra 25
Synopsis: Hardware/PROM: Sun Ultra 25 Flash PROM Update
Date: Sep/22/2009


Install Requirements: None                      
                      
Solaris Release: 10

SunOS Release: 5.10

Unbundled Product: Hardware/PROM

Unbundled Release: OBP 4.30.4, POST 4.30.4, OBDIAG 4.30.4

Xref: 

Topic: 

Relevant Architectures: sparc

BugId's fixed with this patch: 4794955 5079065 5079227 6181985 6183557 6346885 6379703 6381064 6392873 6394040 6431870 6438159 6457354 6458997 6463668 6465220 6470888 6474333 6474932 6478131 6478437 6478646 6480389 6481980 6484677 6484976 6485717 6485941 6487271 6487277 6487287 6487292 6487301 6487332 6487343 6487348 6487438 6487708 6488846 6488855 6490115 6491132 6494774 6494859 6495912 6498373 6498780 6500285 6500287 6500325 6503261 6504355 6504375 6505653 6505657 6505760 6506771 6508437 6508449 6508466 6508474 6508906 6510676 6510693 6510722 6511659 6511901 6512278 6512280 6512314 6512782 6512892 6513595 6515491 6516619 6517108 6517207 6518846 6518865 6518879 6518883 6519920 6519943 6520058 6520718 6521186 6521198 6521605 6521645 6523024 6523823 6524613 6525090 6525913 6526107 6526454 6526699 6526861 6526870 6527778 6528635 6528667 6529207 6529467 6529504 6529934 6532334 6534028 6534031 6535840 6537035 6538367 6539675 6540632 6543430 6543748 6543749 6545197 6545200 6545566 6546593 6547428 6548060 6549753 6550351 6550398 6550717 6550743 6550784 6551724 6553004 6554358 6557874 6558342 6559998 6561842 6561957 6566732 6569526 6570315 6570779 6572821 6573367 6573618 6574092 6574105 6575253 6576406 6579294 6580761 6581085 6581490 6581660 6581794 6583392 6585340 6586400 6587533 6588214 6589154 6589571 6590254 6590384 6590912 6592973 6592986 6593097 6593547 6594395 6594929 6595500 6596546 6596594 6598829 6600945 6601551 6601822 6604051 6604845 6605782 6606197 6608466 6609024 6609130 6611798 6612022 6612178 6616363 6617193 6621175 6622444 6622775 6623111 6623916 6626045 6628699 6629201 6631330 6631946 6633009 6634169 6634974 6634977 6634980 6636978 6638534 6638972 6640485 6644446 6646461 6646532 6646995 6647462 6647984 6650227 6650783 6651513 6652016 6652046 6654860 6654865 6655556 6656072 6657721 6660206 6661787 6662162 6664365 6665538 6666961 6669255 6669488 6670340 6671070 6672367 6674578 6675519 6675677 6675793 6676561 6677840 6678885 6678924 6681061 6682845 6683328 6684123 6684913 6686172 6687097 6688605 6689868 6690618 6690844 6690952 6690978 6693035 6693734 6693906 6694304 6694387 6694497 6697436 6698815 6704491 6705064 6705118 6706303 6706473 6708044 6708234 6708608 6710322 6712358 6712366 6712395 6712683 6713501 6716256 6717373 6719274 6719316 6719407 6720177 6720401 6720575 6721020 6721347 6724265 6725256 6725717 6726148 6728454 6729529 6730281 6730282 6730722 6731112 6732222 6732265 6734408 6735506 6736372 6737081 6737476 6737895 6738373 6739392 6740949 6743825 6747230 6747621 6750734 6751051 6753562 6754453 6755425 6755818 6756295 6760186 6762055 6766240 6770610 6772664 6774655 6777379 6780222 6782337 6787965 6790291 6791196 6791232 6795793 6797789 6802075 6803726 6804349 6807094 6807927 6808167 6809434 6810138 6810143 6812437 6813603 6813715 6816141 6819881 6821770 6825151 6830927 6835857 6835860 6836888 6836962 6839482 6842259 6842274 6855840 6855850 6855865 6858855 6859020 6859443 6860195 6862099 6862229 6866918 6868081 6869577

Changes incorporated in this version: 

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

flash-update-SunUltra25
unix.flash-update.SunUltra25.sh

Problem Description:

6869577 Insufficient memory allocated to the resolution buffer in the ast fcode.
6868081 Probe for TPM support in OpenBoot
6866918 Memory leak in SAS/SATA test 
6862229 speedup of mailbox test
6862099 Multiple resets observed
6860195 Add support to dump PLX FW from DEMON menu
6859443 POST sometimes picks the wrong channel in single channel mode
6859020 POST register assumption
6858855 Integrate AST2100 Fcode into source tree
6855865 Need to increase hotplug-memsize and hotplug-mem64size
6855850 Need to extend the Maximum PCI probe depth
6855840 Add the PCIe Root Port support for RCs containing RPs.
6842274 Speed up of L2 caches tests
6842259 Some of the internal L2 arrays are not being fully tested
6839482 Need to remove clock-divisors from v445
6836962 Various errors reported during Tenaya P1.0 POST HDD testing, thought to be related to FMODs
6836888 Bootblock code in Solaris 10 Update 5 or earlier is incompatible with OpenBoot 4.30 or later
6835860 POST timed out sometimes occurs
6835857 chip reset error occurs when OS boots
6830927 Some healthy components was disabled by a faulted DIMM
6825151 OBP console chars are dropped/scrambled with USB keyboard
6821770 POST error occured on Neptune XAUI 10G Loopback Test
6819881 Didn't receive RTR pkt! when powercycling huron and maramba systems
6816141 virtual storage devices are not getting created under OBP
6813715 POST Niu and Neptune Code Merge
6813603 POST thread bottleneck
6812437 DEMON selectable Systest BusFS causing NoData UEs
6810143 FMOD failures in POST SAS/SATA device test
6810138 Tenaya POST Support
6809434 OBP handles all resumable errors as request to shutdown
6808167 DEMON selectable Systest General test subtest conflict
6807927 VF System keeps power cycles and can't go to obp after POST test done
6807094 Congo:Need OBP changes for Firmware Progress State Sensor
6804349 DVD will not boot -- OBP fix missing to compliment CR 4976792 (READ RETRY)
6803726 Tenaya system (more than 1) hits fbr errors during Enhanced Memory testing
6802075 POST ops1 failed "FATAL ERROR 3", "Unexpected Trap" on N2 systems
6797789 Confusing error messages when using PCIe cards with 64 bit prefetchable BAR
6795793 POST look for display device on T6320
6791232 Monza: Need OBP changes for Firmware Progress Sensor
6791196 POST fails NIU Link Check Test w/ P1 Copper XAUI
6790291 Glendale/Scottsdale need to support REM-less operation
6787965 At post sequence, a CPU core was disabled by mistake, when a faulted DIMM was installed
6782337 POST disk test fails on phy7
6780222 The neptune fcode driver would break if bufsz0 were not set to 2K
6777379 Post support for T6320 G2
6774655 POST loops with "ERROR: No good memory bank/channel left in system" 
6772664 WARNING: /pci@7c0/pci@0/pci@1/pci@0/isa@2: Could not open asr package
6770610 Node Reconfig 2P with CPM1 and CMP3 ERROR: POST timed out. Not all system components tested.
6766240 DVD boot read failures from obp prompt (intermittent DVD DRIVE MISIDENTIFIED may be seen)
6762055 Booting from SATA DVD drives under LSI1068 fails
6760186 queue_tests_timed() function fails to complete under some conditions
6756295 Add support to test serial port from DEMON menu
6755818 Corruption of "my-self" causing missing "idprom" property in root node
6755425 More POST threads starting than expected
6754453 Maramba POST intermittently fails during the 100 power cycle with an LDOM created primary domain.
6753562 Failures of a secondary CMP master are not handled properly
6751051 POST reports hundreds of free resource timeouts
6750734 continuous output of "ERROR: Failed to send a fma event(rc=11)" during POST
6747621 RN50 fcode needs to support new memory
6747230 "1:4:0>ERROR: TEST = PIU intx interrupt test" is output during POST
6743825 POST menu IO-Bridge unit dump causes a crash
6740949 POST Block Mem Schmoo Test is N1 only
6739392 reset host causes POST to fail GBE tests
6738373 Correct Cheetah+ erratum 34 DTLB issue in Starcat OBP
6737895 Some non-critical Neptune/NIU FCode clean up
6737476 OpenBoot disk label package fixes are mising from the large disk support changes
6737081 POST fails PIU PCI id test with ARTM
6736372 DVD boot error from IOU#2 or IOU#6 on DC machines generates wrong error log
6735506 POST is mis-handling a FBR error, if the FBR occurs too early in POST
6734408 Support change from remote-keyboard to rkeyboard in OBP
6732265 POST failures
6732222 nodefault-bytes is not persistent
6731112 Default case in init-xmac-xif sets mii-gmii-mode incorrectly 
6730722 LDOM Device RESET Control reg. is programmed with Maramba value in Scottsdale.
6730282 link up status message includes confusing "duplex = 0"
6730281 netboot via Maramba's Neptune port2 or 3 fails if a copper XAUI is plugged in
6729529 Product definition cleanup
6728454 remove support for N2 erratum 106
6726148 Power-cycling approx. 10 times causes disk devices to disappear.
6725717 V480 onboard CE failed OBDiag test intermittently
6725256 Miscellaneous fixes for OPL platforms
6724265 Initial PUTBACK of Scottsdale Blade to 4.28 and 4.x Gate
6721347 POST fails when X4447A-Z card present in slot PCIE3 or slot PCIE7
6721020 OpenBoot should handle "shutdown" request from Hypervisor
6720575 Add OBP support for Scottsdale Platform
6720401 POST should not fail the GBE device unless it is absolutely certain that the GBE is at fault.
6720177 POST fails with CMP0 missing on T5440
6719407 'Device:' is output 5 times after reset-all on OBP
6719316 USB Failure in POST indicts wrong device
6719274 Thrasher does not work on VF platforms
6717373 cpu-table should be clean before use
6716256 Thunder needs to pick updated OBP which has Scottdale fixes
6713501 Improve PCIE test and scan from post menus.
6712683 POST mistake the slot of the faulted DIMM
6712395 POST times out with 8GB FBDIMMs
6712366 Monitor preferred resolution does not work
6712358 POST print function confusion
6710322 Turgo POST fails when T1 PCI-X card is pluged in
6708608 master cpu timeout occuring on T5140/T5240
6708234 Glendale - watch-net-all terminates and jump by itself to OK when is looking at /niu@80/network@0
6708044 ipmi driver regression: broken on s10u3
6706473 post fails with 3-way config
6706303 post interrupt test fails on n1 platforms
6705118 Intermittent XAUI Lane Synchronization Failure at Flex.
6705064 cr 6705064 POST, block memory test fails if thread 0 is asr disabled
6704491 OBP doesn't display all disabled devices
6698815 POST interrupt test updates
6697436 1G won't work if on Goa if a Goa in slot 1 is not inserted
6694497 POST incorrectly reports timeouts
6694387 OBP will try to run 10G copper at 1G
6694304 DMA function fails
6693906 probe-scsi-all generates Fast Data Access MMU Miss
6693734 Platforms that support MEM64 and PCI hotplug are using invalid memory sizes
6693035 Thunder POST still refers to non existent XAUI ports
6690978 Incorrect diagnosis of a memory UE
6690952 POST code implementation of Node reconfigure for T5440
6690844 Confusing PCIID test error messages
6690618 niu reset from guest doesn't properly prepare niu for 10g mode after running in 1g mode
6689868 With FW 7.1.3_build_02 "boot net - install" doesn't work
6688605 flx22610: Jade host hangs on a reboot with message ERROR: motherboard SEEPROM access failed
6687097 virtual-console device always returns NUL the very first character
6686172 TPM code incorrectly included in Congo POST makefile
6684913 Optimise enhanced POST Systest tests for N2 products
6684123 On OPL OBP can cause OBP to Display incorrect information
6683328 failure of some io devices disabled incorrectly
6682845 2 Unexpected trap37 when running memory screen
6681061 POST support for Thunder platform
6678924 Link width issue with plx version BC chip on pelton 
6678885 Link width issue with plx version BC chip on pelton
6677840 Enhanced POST memory tests on VF platforms should test local memory only
6676561 Changing NVRAM parameter at OS level causes panic : BAD TRAP: type=31
6675793 post hangs if diag verbosity=debug
6675677 POST membist test fails when CH0/D0 is disabled on a branch
6675519 Problem with LSB Degradation
6674578 Sparse CPU support for cpu-struct table
6672367 If a cmp has missing threads/cores in N1, then post will not test some regions of memory
6671070 POST diagnoses to a wrong dimm if a faulty dimm is in either D2 or D3 slots
6670340 Optimise enhanced POST memory tests for N2 products
6669488 POST times out with verbosity min
6669255 Domains fail to boot from the right devalias name
6666961 max level POST on Batoka with memory CE's gets unexpected trap to address 0
6665538 Ikkaku platform support
6664365 flx20948: CP2500 boot-device can be corrupted with a bad read from the AC
6662162 watch-net-all not testing interfaces
6661787 POST support for Batoka
6660206 Huron POST spelling error: "Lopback" missing an "o". eg:"ERROR: TEST = BCM8704 Internal Lopback".
6657721 POST should offline the failing DIMM module in the event of a CE.
6656072 post cpu tests failures, hardware under test is wrong field may state/fail wrong core
6655556 Updated P3 congo/post POST Support for Congo
6654865 OBP development for xaui copper
6654860 POST code setup for xaui copper
6652046 XAUI Conflicting error message
6652016 Sun Blade T6320 has no XAUI
6651513 version negotiation in obp's vnet/vdisk doesn't adhere to the protocol
6650783 PCI Probe error messages could cause problems
6650227 bootmode reset_nvram fails to reset obp to defaults
6647984 Thunder platform support in OBP.
6647462 Problem with T2000 SysFW 6.5.5, won't see DVD rom device after upgrade
6646995 POST output does not appear to be correct - POST is not correctly using SC's diag_<var> values
6646532 OBP providing incorrect compatible property at CPU node
6646461 OPL OBP Update copyright dates to reflect 2008
6644446 POST does not offline by thread when failing tests
6640485 post for maramba needs to be in 4x release gate
6638972 wanboot very slow on maramba
6638534 Maramba 2U with memory config. 24G and 48G on the mezzanine riser does not boot up the server.
6636978 setting input/output device via ok prompt to keyboard/screen results in ERROR: message
6634980 Possible Data corruption when using NVRAMRC kill or yank
6634977 POST run in max mode fails with PLX 8112
6634974 Incorrect Error reported on nvramrc CRC Error
6634169 flx22265: JLL13: no power-off on hotswap causes mcnet to fail to come up on Jade satellites
6633009 Can't boot off XAUI card on Maramba
6631946 (init-program) causes illegal instruction trap if executed when cwp is not 0
6631330 niu driver changes for goa
6629201 maramba post dimm failures must call out the right dimm
6628699 OBP needs to support Maramba platform
6626045 Update Huron RNG OBP virtual-device node
6623916 Software guest state updates generate too much traffic
6623111 Huron system hung after completed POST with "Failed to set device address: 1" with FW 7.0.7
6622775 Running POST with the Neptune FEM installed, disables the PCI-SWITCH
6622444 Boot path switch feature is not work correctly during bootblock load
6621175 False NIU FZC XMAC   Block Port 1 init test failure - RXMAC STATUS Reg. PHY_MDINT Bit
6617193 POST offlines all L2 banks when it encounters a storm of DSC/FBRs
6616363 Glendale's onboard port was not recognized when a Northstar QGC EM card was loaded into the system
6612178 Rev52 Jasper320 cards with v1.13 FCode fails on all Sun platforms
6612022 N1 POST hangs during Enable L2 Cache
6611798 POST support for Turgo
6609130 Monza platform support in OpenBoot
6609024 FERG marks some e-reports from post as invalid and drops them
6608466 GD Post nac names are incorrect
6606197 remove product name from host flash version display
6605782 OBP needs to support the Glendale platform
6604845 Banner does not display the official platform names 
6604051 POST Support for Monza 
6601822 USB hub, keyboard, and/or mouse disappear from OBP device tree
6601551 Use mailbox for systest arguments
6600945 power-off doesn't power off the virtual machine OBP is running within
6598829 ( logo-addr logo-len ) " oem-logo" $setenv is not persistent
6596594 After resetsc, changing OBP nvram parameters do not take affect
6596546 Montoya: "probe-ide" shows a non-existent device with garbage characters as ATAPI model
6595500 Last Trap: Fast Data Access MMU Miss on VDS stress tests
6594929 sun4v systems lost their scsi initiator settings after upgrade to 6.4.x+ firmware
6594395 "Options: true false" menu interrupts OBP reset
6593547 IO-Domain-Reset: ERROR: Last Trap: Watchdog Reset
6593097 POST needs to support SEL_LO_ADR=1 memory addressing
6592986 Add Unix flash update support for U45 MB_PN's 375-3552 and 375-3553 and U25 MB_PN 375-3556
6592973 sata_drive Block error in Hitachi SATA HDDs occurred when power is cycled by s99zzzpc script
6590912 POST needs to clear the FBD syndrome status register twice because of N@ errata #116
6590384 V125(El paso): Could not read diag-level from NVRAM!
6590254 POST is wrongly ASR disabling NIU port in a Single XAUI configuration.
6589571 On OPL XIR at ok? prompt can cause OpenBoot to hang on systems with a large number of strands
6589154 Unexpected traps, L2 UE and lots of error messages in POST when it is faced with FBUs
6588214 Need to remove clock-divisors from v440
6587533 HV Abort: <Unknown?> (82859d0) - PowerDown when starting guest domain that owns bus pci@780
6586400 CR 6554358 breaks builds for excalibur in 4.26.x, 4.25.x,& 4.23.x
6585340 uadmin 2 0 and reboot reads old bootmode settings (should be cleared)
6583392 POST timeouts during PCIE probing (plx errata #7)
6581794 NVRAM configration variable to enable/disable Relaxed Ordering attribute (attr_RO)
6581660 Remove "FBR Error Tally" message in normal verbosity mode
6581490 ERROR: Slave timeout waiting for 6:7 to finish, offlining core 6!
6581085 Can't boot over XAUI network interface
6580761 OBP MMU miss handlers not correct for sun4v spec
6579294 Enhancements to Systest (test within debug menu)
6576406 POST does not run correctly with disabled L2 cache banks[0-3]
6575253 POST needs to report cpu status by strand
6574105 Issuing a boot to the cdrom device hangs the system if no cdrom media is installed
6574092 change post threshold for fbr screen
6573618 Unused POST code
6573367 Disabling cpu8, disables core1 with failed device:MB/CMP0 (CORE) MAU (ERROR: TEST = MAU GF2M MODEXP) 
6572821 Support FWARC 2007/354.
6570779 post reporting 1/2 of available memory while vbsc and solaris report full amount, 4GB memory only
6570315 Post support for Glendale 
6569526 V445 ships with incorrect devalias paths to interval drives when configured with LSI1068e
6566732 IO operation fails randomly after switch-cpu
6561957 OBP bge ethernet driver needs performnace improvement when load a big file (wanboot 108 MB)
6561842 Putback n2-devel gate into 4.x
6559998 Fix to cr 6520058 can cause FORTH stack corruption. 
6558342 POST ends prematurely after "Copy POST to memory"
6557874 Need clean CP2500 OBP smc kcs interface
6554358 Panther L3Tag failures require a POST base test to be detected 
6553004 Hotplug needs to be enabled on St. Paul
6551724 Booting from DVD on Huron fails.
6550784 Data corruption due to wrong sTLB mapping
6550743 (RFE) Jupiter processor support for OPL platforms
6550717 reset.bin too big. Change the N1 POST PROM offset from 1M to 2M
6550398 flx17584: Observed "/console: error to writing to console"
6550351 Issuing a boot to the cdrom device hangs the system if no cdrom is installed.
6549753 Montoya RTM needs support booting from USB disks.
6548060 Add support in 4.x for N2 based platforms
6547428 the warning message has an incorrect spelling. WARNING: No response from Domain Service "Providor"
6546593 WANboot should not reflect packets
6545566 Sun4v call for dma-sync with zero-length buffer results in hypervisor errors
6545200 OpenBoot should only start CPUs which are part of a domain, as indicated by MD
6545197 OpenBoot should use HV API CPU_YIELD when looping in slave loop
6543749 guest domain : wanboot "miniroot" download takes more than 30 minutes
6543748 gust domain : ERROR: Last Trap Memory Address Not Aligned when "watch-net-all" is interrupted
6543430 OBP should retry a cpu_send_mondo hcall if EWOULDBLOCK is returned
6540632 Need definition of OBP power-off for LDOMs systems
6539675 Fix bugs in Systest (performance counter overflow and malloc_bank for half pop systems)
6538367 Huron ophir eeprom mac address is not getting programmed properly with ILOM
6537035 NIU FCode driver needs to clear remote_fault_detected bit (new for N2 2.0 parts)
6535840 POST needs to implement support for ops-mode
6534031 Stack error in NIU FCode driver
6534028 Unable to boot from NIU port 1 (XAUI0)
6532334 When LDOMs had trouble loading up properly, serial port is unusable
6529934 IO device probing on sun4v platforms needs to be hardware agnostic
6529504 Dropping to ok prompt via send break from running OS causes red state exception
6529467 POST should handle preceeding spaces gracefully
6529207 Compile time complaint in USB2 FCode
6528667 vnet FCode should restrict use of MAC address other then local-mac-address
6528635 Changes to speed up dmake have caused lint_check.pl to misreport
6527778 Net installation of multiple domains results in a hang due to out of order packets.
6526870 OBP should automatically create devaliases based on the devalias properties given by zeus
6526861 St Paul SAS WWID should not be programmed based on system-mac-address at run time.
6526699 Doing a build on all products out of the POST tree is very slow
6526454 St. Paul POST has PCI-EM slots reversed
6526107 St. Paul needs to support booting from USB disks.
6525913 "SUN PROPRIETARY/CONFIDENTIAL" message appears on boot on FCS seattle
6525090 reboot-info can be lost on MD updates
6524613 OpenBoot does not handle LDC resets properly
6523823 St. Paul: EM -> PCI-EM
6523024 the /ebus@800 device nods should not show up in domains that do not also have /pci@780
6521645 vdisk drivers should add a more conservative timeout when waiting for handshake packets
6521605 vbsc times out while waiting for POST progress updates to the sequencer and gets reset
6521198 Incorporate enhanced POST memory tests in POST debug menu
6521186 Incorporate new Systest/Thrasher test in POST debug menu
6520718 OBP should assign MAC addresses to on-board network adapters based on MD info from SP
6520058 Schizo FCode driver does not support CDMA interrupts which can lead to Solaris panic
6519943 after upgrading to fw 6.4.0.build_06, OBP NVRAM parameter "security-mode" gets corrupted
6519920 flx20277: UTP - JLL9.2 OBP firmware breaks Jade/UTP tpdriver attachment, 2 UTP env.
6518883 flx20174: obp command, "test-all", hangs on Jade Jalapeno host & satellite.
6518879 St Paul: POST dimm typo
6518865 St. Paul: PEM -> EM
6518846 St. Paul: PEM -> PCI-EM
6517207 LDOMs OBP commands setenv, set-defaults, set-default to not work
6517108 OBP shouldn't be hard-coding max-#cpus
6516619 OPL showdomainstatus incorrectly reflects real state in XCP 1014
6515491 security-mode has a "Default Value" of "none" instead of "No default".
6513595 OBP needs to support the Sun Blade T6300
6512892 Remove IPMI console abort to workaround 'Memory Address not Aligned' trap on Jade
6512782 Ophir EEPROM reprogramming must be enabled on all platforms
6512314 Jade obp shows 'Don't know the role!' after halt
6512280 Add Device ID for new Shrink DIE of Sansung E$ SRAM to POST device database (POST allows device).
6512278 NIU FCode device driver putback
6511901 Jade console hits 'Memory Address not Aligned' trap
6511659 The eeprom command does not work when running on the factory-default MD set
6510722 errors are not printed out at OBP, when a device or devices are asr disabled
6510693 Joint copyright for Sun/Fujitsu needs to be changed for the year 2007 for OPL OpenBoot binary
6510676 OpenBoot will not build on Solaris 10
6508906 post and obp build issues
6508474 OPL OBP should refer to LSB bitmap instead of HWD data when syncing NVRAM data on all LSBs
6508466 LSBID of new console (upon console switch) needs to be saved in SRAM
6508449 Need to add "domain id" information to OPL OBP error log structure
6508437 A STICK register parity error leaves OPL OBP in hung state
6506771 OBP has platforms which don't build any more because of PROM growth
6505760 when disable first thread of a core, post fails whole core after poweroff/on with FATAL ERROR.
6505657 OPL OBP should restart the domain upon detecting an Oberon PCI Channel marked with a UE
6505653 OPL OBP should reboot domain when encountering the memory UE
6504375 local-mac-address? parameter for OPL OBP should default to true
6504355 Openboot: non-functional sun4v retained-memory code places limitations on mblock size and alignment
6503261 changing NVRAM paramter at OS level causes panic : BAD TRAP: type=31
6500325 OPL OBP should not check Oberon link status if POST has already degraded because of link-up failure
6500287 Release new OBP image for SESI Products with enhanced Panther 2100MHz timing.
6500285 FW keying is required to support UltraIV+ high power modules.
6498780 "Can't locate boot device" message on OPL FF1 and FF2 - IOU slot 0 might be the possible cause
6498373 POST did not run after system firmware was upgraded to SIV 6.4.0_build_02
6495912 VSW: "WARNING: exceeded number of permitted handshake attempts" or loss of network connectivity
6494859 Device alias for "cdrom" is set to wrong path on DC systems
6494774 Add guest-state support for Niagara platforms
6491132 V445 AC power restoring causes OBP post fail
6490115 OpenBoot vdisk driver should be compliant to VIO specification
6488855 flx18074: ERROR: motherboard SEEPROM access failed
6488846 FF2:jasper320 FCode checksum error during POST
6487708 Strengthen request_resource function by adding spin lock around potential race condition
6487438 LDOMs OBP does not correctly handle zero length ldom variable updates
6487348 OBP needs to implement the ASR domain-service outlined in FWARC 2006/594
6487343 OBP's virtual nexus probing code is inconsistent when looking for the "ino" md property
6487332 Unable to update ldom-variables after a halt one a system without domaining enabled
6487301 sun4v OBP does not track physmax correctly in the event of multiple mblocks
6487292 Jade .alarms timer not running after Solaris halt
6487287 The OBP LDC driver should conform to FWARC 2005/571
6487277 ./dimmCheck hangs intermittently when we have 8 x Samsung dimms in a Chicago system
6487271 Legacy nvram svc-channel support should be removed from sun4v OBP
6485941 OBP times out prematurely during vdisk/vnet boot
6485717 LDOMs OBP: "reboot-command" does not work as described in LDOM 1.0 OBP Design Spec v1.1
6484976 Error exception before cpu-struct is initialized can cause the machine to hang-up
6484677 Add support for USB2 under OBP
6481980 FCodes for double precision math are broken
6480389 "ERROR: /memory: CPU1 Bank 0 DIMMs are from different vendors"
6478646 PCI bridge probing code does not need to execute config writes to nonexistent devices
6478437 sun4u fire fcode driver initializes 32 bit memory list to incorrect size
6478131 compatible properties for sun4v virtual devices are hard-coded in obp
6474932 Seattle/Boston OBP need to define slot-names property
6474333 POST needs to add support for the LDC console protocol
6470888 OBP firmware will not update on N210s with 375-3471 mainboard
6465220 APL/Niagara platforms need multipath boot support
6463668 Add Logical Domain Support to OBP source base
6458997 LSI 1064/1068 FCode Port enable command adding too much time to system boot
6457354 d< is broken
6438159 Seattle OBP needs to support 2UEEL riser card
6431870 IO forwarding ranges not properly shut down in PCI bridge FCode
6394040 OBP doesn't handle low-cost keyboards without bCountryCode byte
6392873 reset-all after asr-clear executed makes OBP ERROR: motherboard SEEPROM access failed.
6381064 System cannot boot with input set to type-7 keyboard plugged into front Ontario T2000 usb port.
6379703 POST for St Paul
6346885 OpenBoot does not handle Non-Resumable Error traps
6183557 forth.exe uses tokenize.exe which violates the SPARC ABI causing a SEGV crash
6181985 local-mac-address of bge interface is seen on pci card when net  NVALIAS is duplicated
5079227 This, ")" in between "Copyright" and "2004", is not in the right place.
5079065 Make OBP support mapping devices into 64 bit address space on PCI-E bus
4794955 POST debug menu's help not implemented

Patch Installation Instructions:
===============================
Please refer to the Install.info file for instructions on updating
the firmware using the files included in this patch.
 
                >>> END <<<

Special Install Instructions:
 

README -- Last modified date:  Tuesday, September 22, 2009

