| » contact hp |
search: |  | more options |
| Supportall of hp US

|  | HP Services Software Patches |

» | software & drivers
» | ask Compaq
» | reference library
» | forums & communities
» | support tools
» | warranty information
» | contact support
» | parts
» | give us feedback
patches by topic
» | DOS
» | OpenVMS
» | Security
» | Tru64 Unix
» | Ultrix 32
» | Windows
» | Windows NT
associated links
» | what's new
» | contract access
» | browse patch tree
» | search patch tree
» | join mailing list
connection tools
» | nameserver lookup
» | traceroute
» | ping
HP Services Software Patches - vaxlmf03_061
    NOTE:  An OpenVMS saveset or PCSI installation file is stored
           on the Internet in a self-expanding compressed file.
           The name of the compressed file will be kit_name-dcx_vaxexe
           for OpenVMS VAX or kit_name-dcx_axpexe for OpenVMS Alpha.

           Once the file is copied to your system, it can be expanded
           by typing RUN compressed_file.  The resultant file will
           be the OpenVMS saveset or PCSI installation file which
           can be used to install the ECO.

    Copyright (c) Digital Equipment Corporation 1995, 1997.  All rights reserved.

    PRODUCT:   OpenVMS VAX

    COMPONENT:  License Utility

    SOURCE:     Digital Equipment Corporation

    ECO INFORMATION:

         ECO Kit Name:  VAXLMF03_061
         ECO Kits Superseded by This ECO Kit: VAXLMF02_061

            NOTE:  VAXLMF03_061 also contains the license support
                   previously supplied by the following NAS kits
                   for OpenVMS VAX, V5.5-2 through V6.1.

                      NASVAX030
                      NASVAX040
                      NASVAXLMF050

         ECO Kit Approximate Size:  288 Blocks
                        Saveset A -  72 Blocks
                        Saveset B -  72 Blocks
                        Saveset C -  72 Blocks
                        Saveset D -  72 Blocks

         Kit Applies To:  OpenVMS VAX V5.5-2, V5.5-2H4, V6.0, V6.1
         System/Cluster Reboot Necessary:  Yes

    ECO KIT SUMMARY:

    An ECO kit exists for the License Facility on OpenVMS VAX V5.5-2 through
    V6.1. This kit addresses the following problems:

    Problems Addressed in VAXLMF03_061 for OpenVMS VAX V5.5-2,
      V5.5-2H4, V6.0 and V6.1:

      o  Due to an image build error, the VAXLMF02_061 ECO kit
         images did not correct the problems outlined in the problem
         description.

    Problems Addressed in VAXLMF02_061 for OpenVMS VAX V5.5-2,
      V5.5-2H4, V6.0, V6.1:

      o  The OpenVMS Group Table ECO enables additional functionality
         for Concurrent Use License PAKs and Distributed Interactive
         User License PAKs.  This ECO may be duplicated and used with
         each valid OpenVMS Concurrent Use License or Distributed
         Interactive User License.  Customers are allowed to install and
         use the ECO under their existing license agreement.  The
         functionality enabled by this ECO is provided as a courtesy
         to our previously licensed customers.

         Functionality Enabled by the OpenVMS Group Table ECO

      o  The OpenVMS Group Table ECO will enable the OpenVMS
         Concurrent Use License (QL-MT3A*-3*) to run on OpenVMS VAX
         Version 5.5-2 through OpenVMS VAX Version 6.1.

         Without the ECO, the OpenVMS Concurrent Use License works
         on OpenVMS VAX and Alpha systems running OpenVMS Version
         6.2 or greater.

      o  The OpenVMS Group Table ECO will enable the OpenVMS VAX
         Distributed Interactive User License (QL-09SA*-B*) PAK to
         run on:

          -  An OpenVMS Alpha system running OpenVMS Alpha
             Version 6.1 or greater

          -  A mixed OpenVMS VAX and Alpha cluster running
             OpenVMS VAX Version 5.5-2 or greater and OpenVMS
             Alpha Version 6.1 or greater

          -  An OpenVMS VAX system running OpenVMS Version
             5.5-2 or greater

          Without the ECO the OpenVMS VAX Distributed Interactive
          User License works on OpenVMS VAX systems running OpenVMS
          Version 6.0 or greater and will work on OpenVMS VAX and
          Alpha systems running Version 6.2 or greater.

      o  The OpenVMS Group Table ECO will enable the OpenVMS Alpha
         Distributed Interactive User License (QL-MT3A*-B*) PAK to
         run on:

         -  An OpenVMS VAX system running OpenVMS VAX Version
            5.5-2 or greater

         -  A mixed OpenVMS VAX and Alpha cluster running
            OpenVMS VAX Version 5.5-2 or greater and OpenVMS
            Alpha Version 6.1 or greater.

         Without the ECO the OpenVMS Alpha Distributed Interactive
         User License works on OpenVMS Alpha systems running Version
         1.5 or greater and will work on OpenVMS VAX and Alpha
         systems running Version 6.2 or greater.

    INSTALLATION NOTES:

    In order for the corrections in this kit to take effect, the system
    must be rebooted.  If there are other nodes in the OpenVMS VAXcluster,
    they must also be rebooted in order to make use of the new images.

    KEYWORDS ADDED FOR QUERY PURPOSES:

    OPENVMS-ALPHA-ADL
    ADL-USER
    ADL
    VMS-USER
Files on this server are as follows:
    »vaxlmf03_061.README
    »vaxlmf03_061.CHKSUM
    »vaxlmf03_061.CVRLET_TXT
    »vaxlmf03_061.a-dcx_vaxexe
    »vaxlmf03_061.b-dcx_vaxexe
    »vaxlmf03_061.c-dcx_vaxexe
    »vaxlmf03_061.d-dcx_vaxexe

privacy statement | using this site means you accept its terms |
© 1994-2002 Hewlett-Packard Company