| » contact hp |
search: |  | more options |
| Supportall of hp US

|  | HP Services Software Patches |

» | software & drivers
» | ask Compaq
» | reference library
» | forums & communities
» | support tools
» | warranty information
» | contact support
» | parts
» | give us feedback
patches by topic
» | DOS
» | OpenVMS
» | Security
» | Tru64 Unix
» | Ultrix 32
» | Windows
» | Windows NT
associated links
» | what's new
» | contract access
» | browse patch tree
» | search patch tree
» | join mailing list
connection tools
» | nameserver lookup
» | traceroute
» | ping
HP Services Software Patches - vaxshad12_u2055
    NOTE:  An OpenVMS saveset or PCSI installation file is stored
           on the Internet in a self-expanding compressed file.
           The name of the compressed file will be kit_name-dcx_vaxexe
           for OpenVMS VAX or kit_name-dcx_axpexe for OpenVMS Alpha.

           Once the file is copied to your system, it can be expanded
           by typing RUN compressed_file.  The resultant file will
           be the OpenVMS saveset or PCSI installation file which
           can be used to install the ECO.

    Copyright (c) Digital Equipment Corporation 1996.  All rights reserved.

    PRODUCT:    Volume Shadowing for OpenVMS

    OP/SYS:     OpenVMS VAX

    COMPONENT:  SHADOW_SERVER.EXE
                SHDRIVER.EXE

    SOURCE:     Digital Equipment Corporation

    ECO INFORMATION:

         ECO Kit Name:  VAXSHAD12_U2055
         ECO Kits Superseded by This ECO Kit:  None.
         ECO Kit Approximate Size:  288 Blocks
         Kit Applies To:  OpenVMS VAX V5.5-2, V5.5-2H4, V5.5-2HF
         System/Cluster Reboot Necessary:  Yes

         Installation Rating:   2 - To be installed on all systems running
                                    the listed version(s) of OpenVMS and
                                    using the following feature(s):
                                    Volume Shadowing.

         NOTE:  In order to receive the full fixes listed in this kit,
                the following remedial kits must already be installed:

                     VAXSHAD09_U2055

    ECO KIT SUMMARY:

    An ECO kit exists for Volume Shadowing on OpenVMS VAX V5.5-2 through
    V5.5-2HF.  This kit addresses the following problems:

      o  During a Bad Block Recovery operation, if the source member of
         the shadow set cannot be found by the SHDRIVER, a SHADDETINCON
         system crash will occur.

    INSTALLATION NOTES:

    In order for the corrections in this kit to take effect, the system
    must be rebooted.  If the system is a member of a VMScluster,
    the entire cluster should be rebooted.
Files on this server are as follows:
    »vaxshad12_u2055.README
    »vaxshad12_u2055.CHKSUM
    »vaxshad12_u2055.CVRLET_TXT
    »vaxshad12_u2055.a-dcx_vaxexe

privacy statement | using this site means you accept its terms |
© 1994-2002 Hewlett-Packard Company