  S3 Trio64V+ (9FX Motion 331) on OpenVMS? 
 The Question is:
 
Recently installed a 9FX Motion 331 (PCI) Graphics
card into my AlphaServer 1200, and now my
VT320 console no longer displays operator
messages. (It did prior to installing the
card.)
 
How can I get my operator's console messages
to be displayed again?
 
 
 The Answer is:
 
  The 9FX Motion 331 is better known as the S3 Trio64V+, or PB2GA-JD.
 
  To enable OPCOM on the console, remember to enable broadcasts on the
  console via SET TERMINAL OPA0:/PERMANENT/BROADCAST, and to set the
  appropriate OPC$ logical names in SYLOGICALS.COM (SYLOGICALS.TEMPLATE).
 
  Many folks prefer to use a serial console line (separate from the
  workstation display) or the DECwindows console application.
 
