  Disabling MOP Services? 
 The Question is:
 
disable MOP service
 
 
 The Answer is :
 
  See the NCP command SET CIRCUIT SERVICE, assuming DECnet Phase IV.  For
  this to work, you will have to have the CIRCUIT set STATE OFF and then
  later STATE ON.  Also see the DEFINE command, to permanently disable MOP.
  For DECnet-Plus, see NCL and the SET MOP commands.  For the LANCP-based
  management of MOP services (on OpenVMS V6.2 and later), please see the
  LANCP command SET DEVICE devicename/MOP=DISABLE.
 
 Answer written or last revised on  21-OCT-2002 
