  Configuring DECwindows Multi-Head? 
 The Question is:
 
How do you configure CDE for mulitiple head workstations ?
 
 The Answer is:
 
  The baseline hardware configuration involves simply installing multiple
  (identical) graphics controllers.
 
  The OpenVMS Wizard prefers to use DECwindows Motif for multiple-headed
  configurations, as DECwindows CDE and its desktop design tends to assume
  a single head is present -- customizations to the background menu and
  explicit specifications of SET DISPLAY and such are required for use of
  the second head.
 
  With DECwindows Motif, the file DECW$MWM_RC.DAT is used to set up the
  menu available on the displays.
 
  To control the orientation of the displays and various attributes, please
  see the SYS$STARTUP:DECW$PRIVATE_SERVER_SETUP.COM and the .TEMPLATE files.
 
