Introduction
Step 1:
Connecting Local Cables
Step 2:
Connecting the Modem
Step 3:
Connecting Power
Step 4:
Start Your Computer
Step 5:
Recording Internet Settings
Step 6:
Reconfigure Your PC
Step 7:
Installing Software
Troubleshooting
DI-701 Step 1: Connecting Cables DI-701 Quick Starter Guide & Networking Basics STEP 1: Connecting Local Cables For a Single Computer: Use the cross-over cable included in the box to connect the local port on the DI-701 to the Ethernet port on your computer. If you do not have an Ethernet port, you will need to install an Ethernet NIC like the D-Link DFE-530TX. For an Ethernet/Fast Ethernet Network: To connect to an Ethernet or Fast Ethernet network, simply connect the local port of the DI-701 to an uplink port on your hub or switch with the included cross-over cable. If the hub or switch does not have an uplink port, purchase a normal straight-through cable and connect to any port on the hub or switch. If you do not currently have a network, but do have multiple computers you would like to have share your broadband connection, you may want to purchase the D-Link DFE-910 Network In a Box .

© 1999 D-Link Systems, Inc. All rights reserved.